# Configure Interface

- ## Configure Ethernet interface with setup

  - IP address
  - Netmask (0 - 0, 1 - 128, 6 - 254)
  - “ip routing” yes; but “no” to all routing protocols
    - Setup command (interactive)
    - #configure terminal
    - cisco(config)#interface eth o
    - cisco(config)#ip address n.n.n.n mask m.m.m.m

- ## configure e0 for row ethernet with Next IP address

  > example: Network 130.65.241.16/29

  > > IP address 130.65.241.19

Previous slide | Next slide | Back to first slide | View graphic version