# Exercise 2 configure ethernet interface

- ## Configure Ethernet Interface

  > router>enable
  > router#conf t
  > router(config)#int eth 0
  > router(config-if)#ip addr 130.65.241.xx 255.255.255.xx
  > router(config-if)#no shut
  > router(config-if)#^z
  > router#sho int eth 0

- ## Check:

  - telnet to the router from one of the 1E PCs in the row.

  Previous slide | Next slide | Back to first slide | View graphic version