# PPT Slide

> Exercise 1 Login into the router

- Connect console cable to the Serial Port

  > Serial connection PC to cisco router console port

- Console
  % minicom [-s] [/dev/ttyS0]
  or
  % cu -l /dev/ttyS0 -s 9600

- power on router, watch the loading messages

- Login
  - Console or Telnet from UNIX
    Password: cisco
    name> enable
    Password: cisco
  - Leave the session: exit

Previous slide | Next slide | Back to first slide | View graphic version